The mission events are not handled in the LowBattery State.

..

769 <NullTransLog> Null transition taken by Machine \_\_\_\_DriverPX4Machine-0

770 FlightControllerMachine: setting home local position, x = 0, y = 0, z = 0

771: <RaiseLog> Machine FlightControllerMachine-0 raised Event \_\_\_\_fc\_ready

772: <StateLog> Machine FlightControllerMachine-0 entering State StandBy

773 FlightControllerMachine: Entered standby mode

774 <EnqueueLog> Enqueued Event < \_\_\_\_SetGeofenceRadius, namedTup : (field\_0: namedTup : (field\_0: 0,field\_1: 0,field\_2: 0,),field\_1: 60,) > in Machine \_\_\_\_GeofenceMonitorMachine-0 by \_\_\_\_FlightControllerMachine-0

...

787 <DequeueLog> Dequeued Event < \_\_\_\_battery\_critical, -480 > at Machine \_\_\_\_FlightControllerMachine-0

788 FlightControllerMachine: Battery critical alarm, current battery remaining -480

789: <RaiseLog> Machine FlightControllerMachine-0 raised Event \_\_\_\_fc\_px4\_battery\_critical

790: <StateLog> Machine FlightControllerMachine-0 exiting State StandBy

791: <StateLog> Machine FlightControllerMachine-0 entering State LowBattery

792 FlightControllerMachine: LowBattery

793 <DequeueLog> Dequeued Event < \_\_\_\_SetGeofenceRadius, namedTup : (field\_0: namedTup : (field\_0: 0,field\_1: 0,field\_2: 0,),field\_1: 60,) > at Machine \_\_\_\_GeofenceMonitorMachine-0

820 <DequeueLog> Dequeued Event < \_\_\_\_gps\_health\_update, namedTup : (field\_0: false,field\_1: 2,field\_2: 2,field\_3: 10,) > at Machine \_\_\_\_FlightControllerMachine-0

821: <FunctionLog> Machine FlightControllerMachine-0 executing Function ignore

822 <DequeueLog> Dequeued Event < \_\_\_\_POrbPublish, namedTup : (field\_0: 15,field\_1: \_\_\_\_vehicle\_ready,field\_2: true,) > at Machine \_\_\_\_POrbMachine-0

823 <EnqueueLog> Enqueued Event < \_\_\_\_vehicle\_ready, true > in Machine \_\_\_\_MissionPlannerMachine-0 by \_\_\_\_POrbMachine-0

...

873 <EnqueueLog> Enqueued Event < \_\_\_\_POrbPublish, namedTup : (field\_0: 3,field\_1: \_\_\_\_local\_position,field\_2: namedTup : (field\_0: 0,field\_1: 0,field\_2: 0,field\_3: 0,field\_4: 0,field\_5: 0,field\_6: 0,),) > in Machine \_\_\_\_POrbMachine-0 by \_\_\_\_DriverPX4Machine-0

874 <DequeueLog> Dequeued Event < \_\_\_\_mission\_arm, null > at Machine \_\_\_\_FlightControllerMachine-0

875: <StateLog> Machine FlightControllerMachine-0 exiting State LowBattery

876: <StateLog> Machine FlightControllerMachine-0 exiting State Init

877: <StateLog> Unhandled event exception by machine FlightControllerMachine-0